**[**TCS3200 Color Calibration Sheet**]**

**For 220121-r3A and r3B, use range of 10mm to 20mm range.**

**2nd = lowest value of color tested, 3rd = highest valuer of color tested.**

**e.g : Green @10mm = 5, green @20mm = 55;**

**2nd value in map() = 5, 3rd value in map() = 55;**